|  |  |  |  |
| --- | --- | --- | --- |
| **Date:**       | Valid From:       | Valid To:       | Blanket permit? [ ]  |
| **1. Contractor(s)** |  | Orientation Completed? |
| Company Name: |       | # of Workers:       | [ ]  |
| Contact Name: |       | Phone #: |       |
| **2. Job** |  |
| Applicable LSD(s): |       |
| Type of Permit:[ ]  Hot Work [ ]  Cold Work | Description of the work to be completed:       |
| **3. Special Instructions** |  |
| [ ]  A pre-job safety meeting is required. Contractor representatives must attend or the permit receiver(s) must relay information. |
| [ ]  Ground disturbance requires completion of a ground disturbance permit and, if crossing another facility, a backfill inspection report.[ ]  Confined space entry requires completion of a confined space entry permit and/or an equivalent form and watchman’s log.[ ]  Isolation (lock out tag out) may require completion of a lock out and/or blind list form. |
| [ ]  Cellular phones and relay-activated horn alerts must be turned off in hazardous areas. |
| **4. Work Site Inspection** | *Contractor should also complete a field level hazard assessment (FLHA)*  |
| Has the work site been inspected? [ ]  Yes [ ]  No – If no, explain why:       |
| **5. Hazard Identification** |
| [ ]  Toxic atmospheres (e.g. H2S)[ ]  Oxygen deficiency[ ]  Flammable gases / liquids [ ]  Energy / ignition source[ ]  Oxygen / air[ ]  Fire & Explosion Hazard | [ ]  Limited access / egress[ ]  Working at heights / falling[ ]  Rotating equipment[ ]  Pressurized equipment[ ]  Excessive noise (greater than 85dB)[ ]  Electrical hazards | [ ]  Excavation / trenching[ ]  Underground equipment / lines[ ]  Overhead electrical lines[ ]  Moving vehicles / equipment[ ]  Fatigue[ ]  Other (see below) | [ ]  Working alone[ ]  Weather / road / lease conditions[ ]  Housekeeping / lighting[ ]  Extreme temperatures[ ]  Exposure to hazardous materials[ ]  Radioactive / NORM |
| **6. Hazard Controls** |
| **PPE** | **Safety Equipment** | **Isolation** | **Atmospheric Testing** |
| [ ]  Standard*(hard hat, fire retardant coveralls, steel toed boots/shoes & safety glasses)* [ ]  Hearing protection[ ]  Safety harness[ ]  Life line[ ]  Fall protection[ ]  Personal monitor[ ]  Respiratory equipment[ ]  SCBA / SABA equipmentSafety Data Sheet (SDS):                | [ ]  Barricades[ ]  Warning signs[ ]  Additional fire equipment[ ]  WHMIS / TDG compliance[ ]  Waste streams managed[ ]  Watch person required[ ]  Other                          **Ventilation**[ ]  Air[ ]  Steam[ ]  Inert gas purge[ ]  Water flood[ ]  Other                 | [ ]  Electrical [ ]  Mechanical[ ]  Locked and tagged[ ]  Blinded or blanked[ ]  Cathodic protection off[ ]  Disconnected[ ]  Depressured[ ]  Drained *(lines open)*[ ]  Vented *(lines open)*[ ]  Drains / sumps (*covered)*[ ]  Equipment grounded[ ]  Emergency systems bypassed | Testing completed? [ ]  Yes [ ]  NoBy:                          Initial readings:O2       (19.5-23% is acceptable)LEL%       (Must not exceed 20% of LEL)H2S ppm       (Must not exceed 10ppm)**Continuous monitoring and/or testing required?**[ ]  Yes [ ]  No**Environmental conditions:**[ ]  Wind? [ ]  Yes Direction:                [ ]  Calm [ ]  Low Humidity (Static Electricity) |
| **Other hazards and controls:**       |
| **7. Emergency Procedures and Incident Reporting** | [ ]  Muster area?       |
| [ ]  Emergency procedures reviewed? | [ ]  Incident reporting reviewed? |  [ ]  Cellular communication possible?[ ]  Yes [ ]  No |
|  **8. Agreement (Please read/review and understand hazards and controls prior to signing). Post or make readily available.** |
| This agreement is valid only so long as work conditions existing at the same time of its issuance continue and expires upon occurrence of any hazard such as gas leak, liquid spill, drastic operating change or environmental conditions. Any worker will have the right to stop the job if there are reasonable grounds to believe that the job is, or likely to become, unsafe. If a worker refuses work, work shall not resume until the permit is renewed and a hazard is addressed. The contractor agrees to abide by all provincial, federal and local laws and regulations governing the work contemplated by this agreement and warrants that its employees and subcontractors are competent to undertake the specified work and will comply with applicable legislation.  |
| **Issuer:***(Pieridae Rep)* |       | Phone: |       | Signature: |
| **Receiver(s):** |
| Name: | Signature: | Name: | Signature: |
|       |  |       |  |
|       |  |       |  |
|       |  |       |  |
|       |  |       |  |
|  **9. Permit Renewal (all conditions of permit must be reviewed and followed):** |
| Conditions that would void this agreement and require revalidation include any emergency, time expired and crew/shift change. |
| [ ] Revalidation Date:       Time:       | Issuer Initials:       Receiver Initials:       (If multiple, indicate above.) |
| [ ]  Permit close out/work complete. Date       Issuer Initials:       |