|  |  |  |
| --- | --- | --- |
| **General Information** | Safe Work Permit (cross reference) |  |
| Facility Location: |  |
| Specific Location: |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **Permit Validation** | Permit Valid:  (Date & Time) | From:  To: | Work Site Supervisor: |
|  | Permit Closed  (Date & Time) | Job Complete  End of Shift  Cancelled | Signature: |

|  |  |
| --- | --- |
| HAZARDS | |
|  | Corrosive, toxic, oxygen deficient or flammable/explosive atmospheres, either as a normal characteristic of the space or because of the work being performed. |
|  | Contaminants entering from other areas via ducts or piping. |
|  | Temperature extremes (hot or cold). |
|  | Electrical shock or ignition of flammable gases from portable lights, tools or associated electrical equipment. |
|  | Injury from mechanical equipment. |
|  | Abnormal weather conditions such as electrical storms or extreme inversions with no wind. |
|  | Operation of equipment and/or work procedures. |

|  |  |
| --- | --- |
| PRE-JOB SAFETY MEETING | |
|  | Pre-job safety meeting should address: planning, hazard review, roles and responsibilities, communication, training qualifications (including use, care fitting and maintenance of respiratory protective equipment), entry plan and rescue plan. |
| ENTRY AND RESCUE PLAN | |
| Entry Plan (attach separate sheet if required):  Rescue Plan (attach separate sheet if required): | |